****

**Enduro Fountain Dispenser Brix Instructions**

**Adjusting Syrup/Water Ratio (Brix)**

1. Remove valve cover and install syrup separator over the diffuser and through the nozzle.
2. Hold cup under the valve and dispense the beverage for 4 seconds.

**NOTE: Water and syrup must be cold before checking ratios.**

1. Adjust carbonated water flow to the desired rate. (For example, 90-100 ml. / 3-3.75 oz. per second) Turn the flow adjuster 1/4 of a turn at a time, and recheck the flow. To increase reading, turn clockwise.
2. Set a syrup flow adjuster to get the desired ratio.
3. Test the valve and adjust until a consistent ratio is delivered 3 consecutive times.
4. Repeat procedure for other valves.